1. Chu, M., Kitanidis, P. K., and McCarty, P. L. (2005). Modeling microbial reactions at the plume fringe subject to transverse mixing in porous media: When can the rates of microbial reaction be assumed to be instantaneous? Water Resources Research, 41(6), 1-15. <https://doi.org/10.1029/2004WR003495.4>.
2. Ham, P. A., Schotting, R. J., Prommer, H., and Davis, G. B. (2004). Effects of hydrodynamic dispersion on plume lengths for instantaneous bimolecular reactions. Advances in Water Resources, 27(8), 803-813. <https://doi.org/10.1016/j.advwatres.2004.05.008>
3. Liedl, R., Valocchi, A. J., Dietrich, P., and Grathwohl, P. (2005). Finiteness of steady state plumes. Water Resources Research, 41, 1–8. <https://doi.org/10.1029/2005WR004000>.
4. Liedl, R., Yadav, P. K., and Dietrich, P. (2011). Length of 3-D mixing-controlled plumes for a fully penetrating contaminant source with finite width. WaterResources Research, 47. <https://doi.org/10.1029/2010WR009710>.
5. Maier, U., and Grathwohl, P. (2006). Numerical experiments and field results on the size of steady state plumes.Journal of Contaminant Hydrology, 85(1-2), 33–52. <https://doi.org/10.1016/j.jconhyd.2005.12.012>.
6. Panagos, P., Van Liedekerke, M., Yigini, Y., and Montanarella, L. (2013). Contaminated sites in Europe: review of the current situation based on data collected through a European network. Journal of Environmental and Public Health, 2013.
7. Van Liedekerke, M., Prokop, G., Rabl-Berger, S., Kibblewhite, M., and Louwagie, G. (2014). Progress in the management of contaminated sites in Europe. Reference Report by the Joint Research Centre of the European Commission, 1(1), 4-6.
8. Hantush, M. M., and Mariño, M. A. (1996). An analytical model for the assessment of pesticide exposure levels in soils and groundwater. Environmental Modeling and Assessment, 1(4), 263-276.
9. Falta, R. W., Rao, P. S., andBasu, N. (2005). Assessing the impacts of partial mass depletion in DNAPL source zones: I. Analytical modeling of source strength functions and plume response. Journal of Contaminant Hydrology, 78(4), 259-280.
10. Marinko Karanovic, Christopher J. Neville, and Charles B. Andrews. BIOSCREEN-AT: BIOSCREEN with an Exact Analytical Solution. Vol. 45, No. 2 GROUND WATER March–April 2007 (pages 242–245).
11. Birla, S., Yadav, P., Mahalawat, P., Händel, F., Chahar, B., & Liedl, R. (2020). Influence of recharge rates on steady-state plume lengths. *Journal of Contaminant Hydrology*, *235*, 103709. https://doi.org/10.1016/j.jconhyd.2020.103709
12. KORA (2008). Leitfaden – NatürlicheSchadstoffminderungenbeiTeerölaltlasten. BeiträgezuAbfallwirtschaft und Altlasten, Band 58. TechnischeUniversität Dresden. 270 pp.
13. Van Genuchten, M. (1985). Convective-dispersive transport of solutes involved in sequential first-order decay reactions. *Computers & Geosciences*, *11*(2), 129-147. <https://doi.org/10.1016/0098-3004(85)90003-2>
14. Srinivasan, V., & Clement, T. (2008). Analytical solutions for sequentially coupled one-dimensional reactive transport problems – Part I: Mathematical derivations. *Advances In Water Resources*, *31*(2), 203-218. <https://doi.org/10.1016/j.advwatres.2007.08.002>
15. Kumar, A., Jaiswal, D., & Kumar, N. (2010). Analytical solutions to one-dimensional advection–diffusion equation with variable coefficients in semi-infinite media. *Journal Of Hydrology*, *380*(3-4), 330-337. <https://doi.org/10.1016/j.jhydrol.2009.11.008>
16. Sanskrityayn, A., Suk, H., & Kumar, N. (2017). Analytical solutions for solute transport in groundwater and riverine flow using Green’s Function Method and pertinent coordinate transformation method. *Journal Of Hydrology*, *547*, 517-533. <https://doi.org/10.1016/j.jhydrol.2017.02.014>
17. Pérez Guerrero, J., & Skaggs, T. (2010). Analytical solution for one-dimensional advection–dispersion transport equation with distance-dependent coefficients. *Journal Of Hydrology*, *390*(1-2), 57-65. <https://doi.org/10.1016/j.jhydrol.2010.06.030>
18. Pérez Guerrero, J. S., Skaggs, T. H., & van Genuchten, M. T. (2009). Analytical Solution for Multi-Species Contaminant Transport Subject to Sequential First-Order Decay Reactions in Finite Media. *Transport in Porous Media*, *80*(2), 373–387. https://doi.org/10.1007/s11242-009-9368-3
19. Pérez Guerrero, J. S., Skaggs, T. H., & van Genuchten, M. T. (2010). Analytical Solution for Multi-Species Contaminant Transport in Finite Media with Time-Varying Boundary Conditions. *Transport in Porous Media*, *85*(1), 171–188. <https://doi.org/10.1007/s11242-010-9553-4>
20. Pérez Guerrero, J., Pontedeiro, E., van Genuchten, M., & Skaggs, T. (2013). Analytical solutions of the one-dimensional advection–dispersion solute transport equation subject to time-dependent boundary conditions. *Chemical Engineering Journal*, *221*, 487-491. <https://doi.org/10.1016/j.cej.2013.01.095>
21. Latinopoulos, P., Tolikas, D., &Mylopoulos, Y. (1988). Analytical solutions for two-dimensional chemical transport in aquifers. *Journal Of Hydrology*, *98*(1-2), 11-19. https://doi.org/10.1016/0022-1694(88)90202-8
22. Batu, V., & van Genuchten, M. T. (1990). First- and third-type boundary conditions in two-dimensional solute transport modeling. *Water Resources Research*, *26*(2), 339–350. https://doi.org/10.1029/wr026i002p00339
23. Chen, J., Liang, C., Liu, C., & Li, L. (2016). An analytical model for simulating two-dimensional multispecies plume migration. *Hydrology And Earth System Sciences*, *20*(2), 733-753. <https://doi.org/10.5194/hess-20-733-2016>
24. Domenico, P. (1987). An analytical model for multidimensional transport of a decaying contaminant species. *Journal Of Hydrology*, *91*(1-2), 49-58. <https://doi.org/10.1016/0022-1694(87)90127-2>
25. Newell, C. J., McLeod, R. K., & Gonzales, J. R. (1996). BIOSCREEN: Natural Attenuation Decision Support System. User's Manual Version 1.3. GROUNDWATER SERVICES INC HOUSTON TX.
26. Cirpka, O. A., Olsson, Å., Ju, Q., Rahman, M. A., and Grathwohl, P. (2006). Determination of transverse dispersion coefficients from reactive plume lengths. Groundwater, 44(2), 212-221.<https://doi.org/10.1111/j.1745-6584.2005.00124.x>
27. Cirpka, O., &Valocchi, A. (2007). Two-dimensional concentration distribution for mixing-controlled bioreactive transport in steady state. *Advances In Water Resources*, *30*(6-7), 1668-1679. <https://doi.org/10.1016/j.advwatres.2006.05.022>
28. Hunkeler, D., Höhener, P., &Atteia, O. (2010). Comments on “Analytical modelling of fringe and core biodegradation in groundwater plumes.” by Gutierrez-Neri et al. in J. Contam.Hydrol. 107: 1–9. *Journal Of Contaminant Hydrology*, *117*(1-4), 1-6. <https://doi.org/10.1016/j.jconhyd.2010.06.009>
29. Gutierrez-Neri, M., Ham, P., Schotting, R., & Lerner, D. (2009). Analytical modelling of fringe and core biodegradation in groundwater plumes. *Journal Of Contaminant Hydrology*, *107*(1-2), 1-9. <https://doi.org/10.1016/j.jconhyd.2009.02.007>
30. Jaiswal, D. K., Kumar, A., Kumar, N., & Yadav, R. R. (2009). Analytical solutions for temporally and spatially dependent solute dispersion of pulse type input concentration in one-dimensional semi-infinite media. *Journal of Hydro-Environment Research*, *2*(4), 254–263. https://doi.org/10.1016/j.jher.2009.01.003
31. Singh, M., Singh, V., Singh, P., & Shukla, D. (2009). Analytical Solution for Conservative Solute Transport in One-Dimensional Homogeneous Porous Formations with Time-Dependent Velocity. *Journal Of Engineering Mechanics*, *135*(9), 1015-1021. <https://doi.org/10.1061/(asce)em.1943-7889.0000018>
32. Yadav, R.R., and Jaiswal, D.K. (2011). “Two-dimensional analytical solutions for point source contaminants transport in semi-infinite homogeneous porous medium.” *J. Eng. Sci. Technol.*, 6(4), 459–468.
33. Leij, F. J., Toride, N., & van Genuchten, M. T. (1993). Analytical solutions for non-equilibrium solute transport in three-dimensional porous media. *Journal of Hydrology*, *151*(2–4), 193–228. <https://doi.org/10.1016/0022-1694(93)90236-3>
34. Batu, V. (1996). A generalized three-dimensional analytical solute transport model for multiple rectangular first-type sources. *Journal of Hydrology*, *174*(1–2), 57–82. <https://doi.org/10.1016/0022-1694(95)02752-1>
35. Leij, F. J., Priesack, E., & Schaap, M. G. (2000). Solute transport modeled with Green’s functions with application to persistent solute sources. *Journal of Contaminant Hydrology*, *41*(1–2), 155–173. <https://doi.org/10.1016/s0169-7722(99)00062-5>
36. CUR/NOBIS (1995) Dutch Research Programme In-Situ Bioremediation. NOBIS, PO Box 420, 2800 AK Gouda, The Netherlands
37. AFCEE, L. (1999). Borden,“. Technology Application of Low Cost Emplacement of Insoluble Organic Substrate for Enhanced In Situ Reductive Dechlorination of halogenated Aliphatic Hydrocarbons: Dover Air Force Base, Delaware.
38. Wiedemeier, T. H., H. S. Rifai, C. J. Newell, and J. T. Wilson (1999). Natural Attenuation of Fuels and Chlorinated Solvents in the Subsurface, John Wiley, Hoboken, N. J.
39. Wabbels, D., and G. Teutsch (2008), LeitfadenNatürlicheSchadstoffminderungsprozessebeimineralölkontaminierertenStandorten. KORA Themenverbund 1: Raffinerien, Tanklager, Kraftstoffe/Mineralöl, MTBE, UFZ and UniversitätTübingen.
40. Werner, P., Börke, P., andHüsers, N. (2008). LeitfadenNatürlicheSchadstoffminderungbeiTeerölaltlasten. KORA Themenverbund, 2.
41. Blum, P., Sagner, A., Tiehm, A., Martus, P., Wendel, T., and Grathwohl, P. (2011). Importance of heterocylic aromatic compounds in monitored natural attenuation for coal tar contaminated aquifers: A review. Journal of Contaminant Hydrology, 126(3-4), 181-194.
42. Schiedek, T., Grathwohl, P., and Teutsch, G. (1997). LiteraturstudiezumnatürlichenRückhalt/Abbau von SchadstoffenimGrundwasser. Bericht des LehrstuhlsfürAngewandteGeologie, Univ. of Tübingen, Allemagne, Germany.
43. Mace, R. E., Fisher, R. S., Welch, D. M., and Parra, S. P. (1997). Extent, mass, and duration of hydrocarbon plumes from leaking petroleum storage tank sites in Texas. Geologic Circular, 97(1).
44. Rice, D. W., Grose, R. D., Michaelsen, J. C., Dooher, B. P., MacQueen, D. H., Cullen, S. J., ... and Marino, M. A. (1995). California leaking underground fuel tank (LUFT) historical case analyses. California State Water Resources Control Board.
45. Newell, C. J., and Connor, J. A. (1998). Characteristics of dissolved petroleum hydrocarbon plumes, results from four studies. Rapport technique, American Petroleum Institute, Washington DC.
46. Stupp, H. D., and Paus, L. (1999). MigrationsverhaltenorganischerGrundwasser-Inhaltsstoffe und AnsätzezurBeurteilung von MNA. Terra Tech, 5(99), 32-37.
47. Teutsch, G., Grathwohl, P. and Schiedek, T. (1997), Literaturstudiezumnatrlichenr¨uckhalt / abbau von schadstoffenimgrundwasser, Technical Rep. Texte und BerichtezurAltlastenbearbeitung 35/97, LandesanstaltF¨urUmweltschutzBaden-W¨urttemberg, Karlsruhe, Germany.
48. Zech, A., Attinger, S., Bellin, A., Cvetkovic, V., Dietrich, P., Fiori, A., ... and Dagan, G. (2019). A Critical Analysis of Transverse Dispersivity Field Data. Groundwater, 57(4), 632-639.
49. Yadav, P. K., Liedl, R., and Dietrich, P. (2013). Influence of source thickness on steady-state plume length.Environmental Earth Sciences, 71(2), 959–964. <https://doi.org/10.1007/s12665-013-2497-6>.
50. Acharya R, Valocchi AJ, Werth CJ, Willingham TW (2007) Pore scale simulation of dispersion and reaction along a transverse mixing zone in two-dimensional porous media. Water Resour Res 43:W10435. doi:10.1029/2007WR005969
51. FAO, 2010
52. British project Network on Natural Attenuation in Groundwater and Soil (NNAGS)
53. Kerdoff et al., 2008
54. [www.natural-attenuation.de](http://www.natural-attenuation.de)